CV1243_Silica pentode


	
	This valve measures 370x180mm (overall frame), 340x100mm (valve)


	Filament voltage
	13.0V

	Filament current
	40.0A

	Max anode voltage
	10kV

	Max screen voltage
	2kV

	Max anode dissipation
	2.5kW

	Total emission
	2A

	Max cathode return current
	2A

	Typical operating conditions

	Anode voltage
	6kV

	Screen voltage
	2kV

	Control grid voltage
	-25V

	Anode current
	60mA

	Screen current
	2A

	Mutual conductance
	3.0mA/V


Connections: Anode at one end, filament and grids the other.


